

# Programming an ATTiny85 with an Arduino

Arduino software: <http://arduino.cc>

Wiring (for programming)



(LED and resistor are optional)




# Boards Manager Installation


This core can be installed using the boards manager. The boards manager URL is:

http://drazzy.com/package\_drazzy.com\_index.json

1. File -> Preferences ((Arduino->Preferences on Mac), enter the above URL in "Additional Boards Manager URLs"
2. Tools -> Boards -> Boards Manager.
3. Search and select "ATTinyCore by Spence Konde" and click "Install".



You need to ‘burn bootloader’ to get it to run at the right speed (8MHz):



Many thanks to:

<https://create.arduino.cc/projecthub/arjun/programming-attiny85-with-arduino-uno-afb829>